**Seizmik Full, Vented Windshield for Polaris General**

|  |  |
| --- | --- |
| Material: | Part Number |
| Uncoated Polycarbonate | 25019 |
| 2-Side Hard Coated Polycarbonate | 25020 |

* **0.220 Thick 2-sided Hard Coated Polycarbonate**—Maximizes visibility while minimizing physical damage to the windshield
* **2 Durable** **Vents**—Made of glass-filled nylon and made to last
* **Gasket Sealed Components**—For protection against wind and water intrusion
* **Glass-filled Nylon Clamps**—Custom designed, super strong, and low profile so they do not interfere with other accessories
* **Fully Adjustable Air Flow**—Easy-to-use louver makes changing the airflow through your vents simple
* **Defog Mode**—Incoming air can be directed at the inside window surface to help prevent fogging
* **No Tools Required**—Easy to turn knobs makes installation a breeze
* **Seizmik Compatible**—Works with Seizmik accessories: mirrors, light bars, etc.
* **Trailerable**—Up to 65mph when properly prepared

Updated 2/14/20