**Seizmik Universal Auto-Style Rear View Mirror**

**Part Number**

|  |  |
| --- | --- |
| 1.75” Clamp | 18050 |
| 2” Clamp | 18052 |

**Features**

* Designed specifically for use on UTVs
* Two ball joints provide the maximum range of adjustment
* Simple, one-screw setup
* Doesn’t interfere with roofs or windshields
* Shatter resistant tempered safety glass and high impact ABS housing
* Convex mirror for wider viewing angles and image stability
* 1.75” or 2” steel bar clamp option for maximum strength and durability
* Styling matches Seizmik Side View Mirrors

Updated 2/7/20:

* **Aggressive Styling**—A finished look that also helps to reinforce the high impact plastic housing
* **Durable Steel 1.75" Clamp**—Designed to provide a strong grip and keep the mirror stable on the roughest terrain
* **Easy Installation**—Simple one screw installation.
* **Huge Convex Viewing Surface**—Minimizes vibration and gives the driver view of everything behind
* **Double Ball Joints**—Maximizes adjustability
* **Not Just for UTVs**—Designed specifically for UTVs, but the Wide Angle Rear View Mirror also works great on boats, tractors and recreational vehicles